**Design Standards Letter**

**Letter Number: P-2020-03**

**Letter Date: 05/07/2020**

**Effective Date: 07/01/2020**

**Section/Plan No.: 203.61, 203.62, 203.63, 203.64, 203.65, 608.00, 616.10**

**Subject: Revised Supplement to the 2019 Missouri Standard Plans for Highway**

**Construction and New Publication of the 2020 Missouri Standard Plans for Highway Construction**

**TO:** All Central and District Offices

**FROM:** Sarah Kleinschmit

**DATE:**  May 7, 2020

**SUBJECT:** Engineering Policy

Standard Plans Letter No. 3, 2020

The Supplemental Revisions to the *2019 Missouri Standard Plans for Highway Construction* and new publication of the *2020 Missouri Standard Plans for Highway Construction,* effective July 1, 2020are now available on MoDOT’s website.

Questions regarding the Supplemental Revisions to the Missouri Standard Plans for Highway Construction should be directed to Rick Prosser, Central Office, Engineering Policy Services, at 573-526-8485 or myself at 573-751-7412.

**REVISIONS:**

**203.61** *(sheet 1 of 1)*. Revised detail for Driveway Typical Section to show Type 1 or 5 Base beneath pavement. Added “4 inches of Type 1 or 5 Base shall be placed and compacted beneath the areal surface of concrete and asphalt driveways.” to General Notes.

**203.62** *(sheet 1 of 2)*. Added “4 inches of Type 1 or 5 Base shall be placed and compacted beneath the areal surface of concrete and asphalt driveways.” to General Notes.

**203.62** *(sheet 2 of 2)*. Revised detail for Driveway Typical Section to show Type 1 or 5 Base beneath pavement.

**203.63** *(sheet 1 of 2)*. Added “4 inches of Type 1 or 5 Base shall be placed and compacted beneath the areal surface of concrete and asphalt driveways.” to General Notes.

**203.63** *(sheet 2 of 2)*. Revised detail for Driveway Typical Section to show Type 1 or 5 Base beneath pavement.

**203.64** *(sheet 1 of 2)*. Added “4 inches of Type 1 or 5 Base shall be placed and compacted beneath the areal surface of concrete and asphalt driveways.” to General Notes.

**203.64** *(sheet 2 of 2)*. Revised detail for Driveway Typical Section to show Type 1 or 5 Base beneath pavement.

**203.65** *(sheet 1 of 1)*. Added “Base” to the second paragraph in Notes.

**608.00** *(sheet 1 of 2)*. Revised detail for Section A-A to show Type 1 or 5 Base beneath pavement. Added “4 inches of Type 1 or 5 Base shall be placed and compacted beneath the areal surface of paved approaches.” to General Notes.

**608.00** *(sheet 2 of 2)*. Revised detail for Section F-F to show Type 1 or 5 Base beneath pavement. Added “4 inches of Type 1 or 5 Base shall be placed and compacted beneath the areal surface of paved approaches.” to General Notes.

**616.10** *(sheet 1 of 9)*. Condensed detail for Height and Lateral Locations for Post and Portable Sign Mounting to clarify flag installation.

**616.10** *(sheet 2 of 9)*. Changed 30 to 32 (sq. ft.) in the 4th row showing Sign Area in the table for Post Type. Added “Sign installation details shown shall apply to all posts in a multi post installation” to General Notes. Removed Optional U-Channel Post detail. Added Post Spacing detail.

SKK/RGP